**Departure Checklist**

* Top-off Fresh Water Tank
* Closet
  + Close Washer/Dryer doors
  + Hang Cover to Back Wall (Shoe Rack)
  + Check Hanging Items are secure
  + Check Doors and Drawers
  + Lock Closet Door
* Rear Bathroom
  + Turn Off Floor Heat
  + Lock Shower Door
  + Be Sure Fan is Off
  + Check Towels are off Shower Wall
  + Stack Bathroom Rugs
  + Low Water Mode
  + Close Toilet Seat
  + Remove Magnetic Lights
  + Remove Bidet Remote
  + Check all Cabinets / Fully Closed
  + Turn off/store dehumidifier
  + Clear Counter Tops
  + Close Sink Drain
  + Lock Bathroom Door
* Bedroom
  + Check Nightstands – put cords on bed
  + Remove Tonya’s Fan
  + Remove Wreath/Decor from Mirror
  + Check compartments under bed
  + Fold comforter up on bed
  + Check Drawers/Cabinets Latched
  + Check Liquor Cabinet
  + Turn Off Floor Heat
  + Lock Bedroom Door
* ½ Bathroom
  + Check all Cabinets
  + Low Water Mode
  + Close Toilet Seat
  + Be Sure Fan is Off
  + Close/Latch Bathroom Door
* Kitchen
  + Check Fridge Contents
  + Lock Fridge
  + Check Pantry Pullouts
  + Remove Small Plants from Mirror
  + Put Silicone Popcorn Popper in Microwave
  + Clear Countertops
  + Cover Cooktop
  + Televator down
  + Check exhaust fan is off
  + Check Lock on Dishwasher
  + Close Dinette Table/Secure Chairs
  + Check Drawers/Cabinets Latched
  + Check Island is locked
  + Put Away Dog Food/Water Bowls
  + Turn Off Floor Heat
  + Turn Off Fireplace
* Front
  + Raise Night Shades
  + Remove Hanging Plants
  + Remove Monster
  + Check Cabin Seats are Clear of Slides
  + Top off Fresh Water Tank
  + Make sure extra steps are stored
  + Unlock Steps
  + Lower Antennas
  + Preprogram Route / Plan Fuel Stops
  + Oasis AC1/AC2 and Burner Off
  + Verify Girard Awnings are unplugged
  + Adjust A/C for Disconnect/Travel
* Starting

\*\*\*Anything under bus?\*\*\*

* Turn Key to “ON” (Don’t crank engine) (Damn beeping starts)
* Wait for yellow “CHECK ENGINE” Light to go off (on dash)
* Start Engine
* Set High Idle (on turn signal slider)
* Wait for air pressure to reach 3/4 on both dials
* Auto-Store Jacks on left panel (damn beeping stops! Yay!)
* Wait for blue light to stop blinking (on Left Panel)
* Check Seats again for Slide Clearance
* Big Slide in First
* Two small slides in. Keep eye on bedroom bedding clearance
* Wet Bay - Sewer
* Open Black Tank Valve (Left)
* Turn on Sanicon
* Wait until done (hose retracts)
* Turn on Tank Rinse Water (valve)
* Wait until clean
* Turn off Tank Rinse Water (valve)
* Open Grey Tank Valve (Right)
* Wait until done (hose retracts)
* Turn off Sanicon
* Put on Gloves
* Empty Stinky Slinky Manually
* Close Grey Valve
* Close Black Valve
* Remove the Stinky Slinky and Cap it
* Put cap on Stinky Hole
* Store Stinky Slinky
* Remove Gloves
* Wash Hands Get extra paper towels when dry hands
* Wet Bay – Fresh Water
* Disconnect Drinking Water Hose from Spigot
* Wrap water hose in paper towels and use power reel
* Disconnect Rinsing Hose from Coach and Spigot
* Drain and Store Rinsing Hose
* Power Bay
* Turn off Circuit Breaker at Pedestal
* Unplug Power Cord from Pedestal
* Wrap Power Cord with Paper Towels and Power Retract
* Exterior Inspection
  + Check Each Bay Door to Ensure Closed/Latched
  + Check Engine Cover
  + Check Generator Slide
  + Check All Awnings
  + Check Roof Antennas
  + Verify Slides Fully Closed Properly
  + Verify All Jacks are Retracted
  + Verify Ride Height
  + Check Tires
  + Check Windows
* Hook up Toad
  + Blue Ox Arms
  + Safety Cables – Hooks Down
  + Power Line
  + Air Line
  + Breakaway Cable
* Flat Tow Mode
  + Turn Key to On, Do Not Start
  + Hold Brake, Put Transmission in Neutral from Park
  + Release Brake, Put Transfer Case in Neutral (Floor)
  + Hold Brake, Put Transmission in Park
  + Turn off Key and Remove
  + Push Hobart Back to Lock Tow Arms
* Final Checks
  + Light Check
  + Check Toad Rolls (all 4 tires)
  + Verify AGS is On
  + Verify A/C is Set for Travel
  + Close Overhead Cabinet