**Departure Checklist**

* Top-off Fresh Water Tank
* Closet
	+ Close Washer/Dryer doors
	+ Hang Cover to Back Wall (Shoe Rack)
	+ Check Hanging Items are secure
	+ Check Doors and Drawers
	+ Lock Closet Door
* Rear Bathroom
	+ Turn Off Floor Heat
	+ Lock Shower Door
	+ Be Sure Fan is Off
	+ Check Towels are off Shower Wall
	+ Stack Bathroom Rugs
	+ Low Water Mode
	+ Close Toilet Seat
	+ Remove Magnetic Lights
	+ Remove Bidet Remote
	+ Check all Cabinets / Fully Closed
	+ Turn off/store dehumidifier
	+ Clear Counter Tops
	+ Close Sink Drain
	+ Lock Bathroom Door
* Bedroom
	+ Check Nightstands – put cords on bed
	+ Remove Tonya’s Fan
	+ Remove Wreath/Decor from Mirror
	+ Check compartments under bed
	+ Fold comforter up on bed
	+ Check Drawers/Cabinets Latched
	+ Check Liquor Cabinet
	+ Turn Off Floor Heat
	+ Lock Bedroom Door
* ½ Bathroom
	+ Check all Cabinets
	+ Low Water Mode
	+ Close Toilet Seat
	+ Be Sure Fan is Off
	+ Close/Latch Bathroom Door
* Kitchen
	+ Check Fridge Contents
	+ Lock Fridge
	+ Check Pantry Pullouts
	+ Remove Small Plants from Mirror
	+ Put Silicone Popcorn Popper in Microwave
	+ Clear Countertops
	+ Cover Cooktop
	+ Televator down
	+ Check exhaust fan is off
	+ Check Lock on Dishwasher
	+ Close Dinette Table/Secure Chairs
	+ Check Drawers/Cabinets Latched
	+ Check Island is locked
	+ Put Away Dog Food/Water Bowls
	+ Turn Off Floor Heat
	+ Turn Off Fireplace
* Front
	+ Raise Night Shades
	+ Remove Hanging Plants
	+ Remove Monster
	+ Check Cabin Seats are Clear of Slides
	+ Top off Fresh Water Tank
	+ Make sure extra steps are stored
	+ Unlock Steps
	+ Lower Antennas
	+ Preprogram Route / Plan Fuel Stops
	+ Oasis AC1/AC2 and Burner Off
	+ Verify Girard Awnings are unplugged
	+ Adjust A/C for Disconnect/Travel
* Starting

\*\*\*Anything under bus?\*\*\*

* Turn Key to “ON” (Don’t crank engine) (Damn beeping starts)
* Wait for yellow “CHECK ENGINE” Light to go off (on dash)
* Start Engine
* Set High Idle (on turn signal slider)
* Wait for air pressure to reach 3/4 on both dials
* Auto-Store Jacks on left panel (damn beeping stops! Yay!)
* Wait for blue light to stop blinking (on Left Panel)
* Check Seats again for Slide Clearance
* Big Slide in First
* Two small slides in. Keep eye on bedroom bedding clearance
* Wet Bay - Sewer
* Open Black Tank Valve (Left)
* Turn on Sanicon
* Wait until done (hose retracts)
* Turn on Tank Rinse Water (valve)
* Wait until clean
* Turn off Tank Rinse Water (valve)
* Open Grey Tank Valve (Right)
* Wait until done (hose retracts)
* Turn off Sanicon
* Put on Gloves
* Empty Stinky Slinky Manually
* Close Grey Valve
* Close Black Valve
* Remove the Stinky Slinky and Cap it
* Put cap on Stinky Hole
* Store Stinky Slinky
* Remove Gloves
* Wash Hands Get extra paper towels when dry hands
* Wet Bay – Fresh Water
* Disconnect Drinking Water Hose from Spigot
* Wrap water hose in paper towels and use power reel
* Disconnect Rinsing Hose from Coach and Spigot
* Drain and Store Rinsing Hose
* Power Bay
* Turn off Circuit Breaker at Pedestal
* Unplug Power Cord from Pedestal
* Wrap Power Cord with Paper Towels and Power Retract
* Exterior Inspection
	+ Check Each Bay Door to Ensure Closed/Latched
	+ Check Engine Cover
	+ Check Generator Slide
	+ Check All Awnings
	+ Check Roof Antennas
	+ Verify Slides Fully Closed Properly
	+ Verify All Jacks are Retracted
	+ Verify Ride Height
	+ Check Tires
	+ Check Windows
* Hook up Toad
	+ Blue Ox Arms
	+ Safety Cables – Hooks Down
	+ Power Line
	+ Air Line
	+ Breakaway Cable
* Flat Tow Mode
	+ Turn Key to On, Do Not Start
	+ Hold Brake, Put Transmission in Neutral from Park
	+ Release Brake, Put Transfer Case in Neutral (Floor)
	+ Hold Brake, Put Transmission in Park
	+ Turn off Key and Remove
	+ Push Hobart Back to Lock Tow Arms
* Final Checks
	+ Light Check
	+ Check Toad Rolls (all 4 tires)
	+ Verify AGS is On
	+ Verify A/C is Set for Travel
	+ Close Overhead Cabinet