**Landing Checklist**

* Driver
  + Engage Parking Brake
  + Put in Neutral
  + Set High Idle
  + Turn Off Lights
  + Check Levelness of Coach (LevelMate Pro)
* Outside
  + Check Slide Gaps/Paint Lines
  + Check Distance for Slides
  + Check Distance for Power, Water and Sewer
* Power
  + Verify Pedestal is off
  + Plug in Surge Protector
  + Turn on Pedestal Breaker
  + Check for Green Lights on Surge Protector
  + Turn off Pedestal Breaker
  + Plug in Shore Power
  + Position Cable so good
  + Turn on Pedestal Breaker
* Wet Bay
  + Connect Water/Turn On
  + Connect Sewer
  + Open Grey Tank Valve
* Slides
  + Remove Slide Towels
  + Check Captain Chairs Clearance
  + Small Slides Out
  + Big Slide Out
  + Auto-Level
  + Turn on AC1/AC2 Hot Water
  + Ensure Auto-Fill is on
* Unhook Toad
  + Blue Ox Arms
  + Safety Cables – Hooks Down
  + Power Line
  + Air Line
  + Breakaway Cable
* Hobart Drive Mode
  + Transfer Case 2H
  + Start Engine, Check Drive