**Landing Checklist**

* Driver
	+ Engage Parking Brake
	+ Put in Neutral
	+ Set High Idle
	+ Turn Off Lights
	+ Check Levelness of Coach (LevelMate Pro)
* Outside
	+ Check Slide Gaps/Paint Lines
	+ Check Distance for Slides
	+ Check Distance for Power, Water and Sewer
* Power
	+ Verify Pedestal is off
	+ Plug in Surge Protector
	+ Turn on Pedestal Breaker
	+ Check for Green Lights on Surge Protector
	+ Turn off Pedestal Breaker
	+ Plug in Shore Power
	+ Position Cable so good
	+ Turn on Pedestal Breaker
* Wet Bay
	+ Connect Water/Turn On
	+ Connect Sewer
	+ Open Grey Tank Valve
* Slides
	+ Remove Slide Towels
	+ Check Captain Chairs Clearance
	+ Small Slides Out
	+ Big Slide Out
	+ Auto-Level
	+ Turn on AC1/AC2 Hot Water
	+ Ensure Auto-Fill is on
* Unhook Toad
	+ Blue Ox Arms
	+ Safety Cables – Hooks Down
	+ Power Line
	+ Air Line
	+ Breakaway Cable
* Hobart Drive Mode
	+ Transfer Case 2H
	+ Start Engine, Check Drive